ecoCentric™ StudentSeat Height [eco-STUDENT]

|  |  |
| --- | --- |
| Backrest* Dual Curve Plastic Back (20”w x 12.5”h)
* Handle in back for easy movement
* Unique Scalloped Indentations for the spine

Back and Seat Frame* 14 Gauge, 7/8” Steel Tube Frame
* Black Textured Semi-Gloss Powder Coat Paint

Seat* 18”w x 18.5”d
* Dual Curve Waterfall Plastic Seat in Black
* Unique Scalloped Indentations for the Seat Bones

**Options:*** Grey Package (Includes Grey Seat and Backrest)
* Upholstered Seat [UPHS]

Seat Height Mechanism* Seat Height

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (14.5" – 19.5")

**Options:*** 80 mm Pneumatic Lift (13.5”-16.5”) [80mm]
* 100 mm Pneumatic Lift (14”-17.5”) [100mm]
* 140 mm Pneumatic Lift (15.25”-20.75”) [140mm]
* 157 mm Pneumatic Lift (17.25”-23”) [157mm]
* 200 mm Pneumatic Lift (Includes upgrade to 26” base for stability) (20.5”-27.5”) [200mm]
* 267 mm Pneumatic Lift (23”-33”) [267mm]
 | Base/Glides/Casters* 24” Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* 20” Diameter Height Adjustable Footring (for use as a foot rest only) [20FR]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]
* 26” Glass Reinforced Nylon Base [26NB]

Additional Options* Grey Plastic Backrest (20”w x 12.5”h) [PLABG]
* Grey Plastic Seat (18”w x 18.5”d) [PLASG]

  |