Industrial SF™Standard [IND SF Standard]

|  |  |
| --- | --- |
| Backrest   * Fully Upholstered Dual Curve Backrest * 15.5" wide by 13.5" high   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * High Resilient Polyurethane Foam * Seat Pan 18.5" wide by 17" deep   **Options:**   * Memory Foam Seat [EA] * Extra small seat - 17.5"W x 15.5"D (Trigger Adjustable T-arms [TATA] recommended with this option) [XSS] * Standard Non-Airflow Seat (20â€w x 19â€d) [LS] * ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS] * Plastic Back Cap II (Fabric Upholstery) [PBCIIF] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]   Standard Mechanism   * Back Angle Adjustment * Back Height Adjustment * Back Pivot   Pneumatic Lift  (Seat Height)   * 200 mm Knurled Pneumatic  Lift, Dual Height Adjustment  System (seat height 7.5" of  adjustment between 21"- 33.5") | Base/Glides/Casters   * 26" Multi-level Spider Base with Durable Urethane Coating * ½" Industrial Glides * Footrests 3", 6.5", 9", 12" high   **Options:**   * 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22] * 30" Diameter Flat Bi-level Footrest (30"W x 20.5"H) [30FBLFR] * Nylon Casters (adds 1.5" to seat height) [NC] * Urethane Casters (adds 1.5" to seat height) [UC] * Single Wheel Casters (adds 1.5" to seat height) [SW] * Single Wheel Urethane Casters (adds 1.5" to seat height) [SWU] * Lock-on Urethane Casters (adds 1.5" to seat height) [LON] * Lock-off urethane casters (adds 1.5" to seat height) [LOF] * 1/2" Flat Glides [HG] * 2 1/4" Glides (adds 1.5" to seat height) [2G]   Upholstery   * Chair in vinyl, fabric or ergoCentric+Guard   Additional Options   * Back Trim [BT] * Cal. 133 [Cal133] * Anti Static (Available in fabric and vinyl only) [ANTISTATIC] * Class 100 Cleanroom (only available in vinyl) [CRPACK] * Height Adjustable Footring [ERGOFR] |