Industrial SF™Standard [IND SF Standard]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest
* 15.5" wide by 13.5" high

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* High Resilient Polyurethane Foam
* Seat Pan 18.5" wide by 17" deep

**Options:*** Memory Foam Seat [EA]
* Extra small seat - 17.5"W x 15.5"D (Trigger Adjustable T-arms [TATA] recommended with this option) [XSS]
* Standard Non-Airflow Seat (20â€w x 19â€d) [LS]
* ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS]
* Plastic Back Cap II (Fabric Upholstery) [PBCIIF]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]

Standard Mechanism* Back Angle Adjustment
* Back Height Adjustment
* Back Pivot

Pneumatic Lift (Seat Height)* 200 mm Knurled Pneumatic Lift, Dual Height Adjustment System (seat height 7.5" of adjustment between 21"- 33.5")
 | Base/Glides/Casters* 26" Multi-level Spider Base with Durable Urethane Coating
* ½" Industrial Glides
* Footrests 3", 6.5", 9", 12" high

**Options:*** 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22]
* 30" Diameter Flat Bi-level Footrest (30"W x 20.5"H) [30FBLFR]
* Nylon Casters (adds 1.5" to seat height) [NC]
* Urethane Casters (adds 1.5" to seat height) [UC]
* Single Wheel Casters (adds 1.5" to seat height) [SW]
* Single Wheel Urethane Casters (adds 1.5" to seat height) [SWU]
* Lock-on Urethane Casters (adds 1.5" to seat height) [LON]
* Lock-off urethane casters (adds 1.5" to seat height) [LOF]
* 1/2" Flat Glides [HG]
* 2 1/4" Glides (adds 1.5" to seat height) [2G]

Upholstery* Chair in vinyl, fabric or ergoCentric+Guard

Additional Options* Back Trim [BT]
* Cal. 133 [Cal133]
* Anti Static (Available in fabric and vinyl only) [ANTISTATIC]
* Class 100 Cleanroom (only available in vinyl) [CRPACK]
* Height Adjustable Footring [ERGOFR]
 |