geoCentric Counter Stool [geo-STOOL]

|  |  |
| --- | --- |
| Backrest* Backrest 18.25" wide by 12.5" high
* Concealed Back Brackets (except when upholstered in vinyl or leather)
* Dual Curve Backrest

Seat* 31.25" Seat Height
* Dual Curve Waterfall Seat
* Seat Pan 18.5" wide by 19.5" deep
 | Base/Glides/Casters**Options:*** Metal Sled base option with glass reinforced nylon glides (SLED)

Frame* 14 Gauge, 7/8" Steel Tube Frame
* Black Textured Semi-Gloss Powder Coat Paint
* Kick Back Legs for Stability with Durable Custom Glides
* Step 12" high

**Options*** Counter stool chrome frame (CCF)

Additional Options* Cal. 133 [Cal133]
* Ganging clips (set of 2) chair with no arms [GCNA]
 |