tCentric Hybrid™

|  |  |
| --- | --- |
| Knee Tilt\* | Midnight Black [t-KT] |
| Backrest:   * 5" Patented Back Height Adjustment System * Dual Curve Mesh Backrest (19"w x 25"h)   Arms:  Midnight Black  **Options:**   * tCentric Armrest Height & Lateral [TCL] * tCentric Armrest Height & Swivel [TC360] * tCentric Armrest Height, Lateral & Swivel [TCL360]   Seat: Midnight Black   * Dual Density Molded Polyurethane Foam * Eight ply hardwood seat structure * Tailored upholstery on seat pan (20”w x 19”d)   **Options:**   * Extra Small Seat (17 ½”w x 15 ½”d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Plus Size Seat (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Extra Deep Seat (22”w x 21”d) [XPS] * Energy Absorbent Memory Foam [EA] * Triple Density Foam (adds ¼” to seat width & depth) [TDF] * Non-tailored Seat Pan [NTS]   Knee Tilt Mechanism:  Midnight Black   * 5” Incremental Back Height * Infinite Lock Free Float * Back Angle * Spring Tension * 2 ½” Seat Depth * Pneumatic Seat Height   Measurements/Overall Dimensions:  Boxed Weight/Size: 46.4 lbs. / 11.7 cu.ft. | Pneumatic Lift (Seat Height): Midnight Black   * 125 mmLT Pneumatic Lift (18 ¾" – 23 ½")   **Options:**  *Midnight Black [G]*   * 70 mm Pneumatic Lift (18 ¼” – 21”) [70MM] * 80 mm Pneumatic Lift (19”-22”) [80MM] * 100 mm Pneumatic Lift (19 ½”-23 ¼”) [100MM/G100MM] * 140 mm Pneumatic Lift (20 ¾”-26 ¼”) [140MM/G140MM]   *Chrome*   * 100 mm Chrome Pneumatic Lift (19 ½”-23 ¼”) [100MMCH] * 125 mm Chrome Pneumatic Lift (19 ¾”-24 ½”) [125MMCH] * 140 mm Chrome Pneumatic Lift (20 ¾”-26 ¼”) [140MMCH]   Base/Glides/Casters:  Midnight Black   * 26" Glass Reinforced Nylon Mid-Profile Base * 5 Dual Wheel Nylon Casters 2   **Options:**   * Chrome Accent Casters [CAC] * 26” Polished Aluminum Mid-Profile Base [PMB] * Dual Wheel Urethane Caster 2 [UC2]   Additional Options:  Midnight Black   * tCentric Lumbar Support [TLS] * tCentric Lumbar Support with Air Lumbar (pump) [TLSAL] * Adjustable Headrest [AHR] |

­